**Comment/Explanation\*:***Include your justification for your proposed change to the draft standard below.*
\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_We suggest that Table 5.3.2 include industry-average EPDs without manufacturer listed should also be in the list of options for how to model a product without a product specific EPDs, though lower on the hierarchy. This is consistent with common practice and with the data hierarchy in the draft standard of ASHRAE 240p presented in *Table 6.2.1 Types of environmental impact data to be used during different modeling Assessments*. The current approach in the RENSET standard should be updated to be clear that an industry-average EPD for comparable product type when product manufacturer is *not* listed on the EPD is also acceptable as a data source.

References: ASHRAE, ICC, & BSR. (2025). Standard 240P: Quantification of Life Cycle Greenhouse Gas Emissions, Second ISC Publication Public Review Draft. ASHRAE.

**Proposed Change to the Draft Standard\***
*Use “strikethrough” and “underline” formatting to indicate all proposed changes. Changes must be shown with “hard-formatting” strikethrough and underline, not “track changes”.*

*Use a color other than red to indicate proposed changes to the draft.*\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Industry-average EPD for comparable product type when product manufacturer is listed on the EPD
2. Industry-average EPD for comparable product type
3. Benchmark value for comparable product type in accordance with section 5.3.3.
4. LCA for comparable product type
5. For MEP products, default values from Table 10.1.5.