RESNET® Standards Public Comment and Proposed Change Form
Comment/Explanation*: 
Include your justification for your proposed change to the draft standard below.
_________________________________________________________________________________________
Commenter: Mathew Ford (mford05@nyit.edu), Managing Director, Center for Offsite Construction (CfOC), New York Institute of Technology
Document: BSR/RESNET/ICC 1550-202x
Section referenced: Section 10, Table 10.2.1 (Waste Rates for Products), Note (c)
Comment 1 — expand the "volumetric modular construction" example to remove ambiguity. Note (c) lists "volumetric modular construction" as a single, unelaborated example among several qualifying for the 0% on-site waste rate. We recommend expanding this line to remove ambiguity about which configurations qualify. (See Comment 1 – Proposed Change, below) 
This preserves the existing criteria-based structure and simply ensures verifiers do not have to guess whether common modular configurations, such as stacked multi-story units or hybrid panel/volumetric assemblies, fall within the intended scope.


Proposed Change to the Draft Standard*
Use “strikethrough” and “underline” formatting to indicate all proposed changes. Changes must be shown with “hard-formatting” strikethrough and underline, not “track changes”. 
Use a color other than red to indicate proposed changes to the draft.
____________________________________________________________________________________________
Comment 1 — Proposed Change (p.32)

Table 10.2.1 Notes:
a) Applies to standardized prefabricated assemblies or equipment that are shipped to site ready to be installed without any alterations resulting in wastage such as cutting or trimming or drilling. For example: standard windows, small appliances.
b) Any additional material to be applied on site such as coatings or connection materials shall be accounted for separately with applicable on-site wastage ratios.
c) Applies to custom prefabricated assemblies meeting all the following: 
· Weighs more than 200 lbs per piece 
· Fabricated to the specific dimensions required for the project. 
· Shipped to site as a kit of parts or as a single piece ready to be installed without any alterations resulting in wastage such as cutting or trimming or drilling. 
· For example: unitized curtainwall, volumetric modular construction (including multi-story stacked modular units, panelized wall, floor, and roof systems, and hybrid assemblies combining panelized and volumetric components), provided the assembly meets the weight and fabrication criteria above, structural steel members, glue-laminated beams and CLT panels, 781 architectural precast panels.
d) Applies to flat products at least 18 inches in two directions. Otherwise use "tiles" or "elements delivered to site in standard length."

