**PDS-01 Addendum 79f**

**Table 5.1.2(1) Informative Note Correction**

***6. Modify the (Informative Note) identified as “1” below as shown:***

**Table 5.1.2(1) Emission Factors for Household Combustion Fuels[[1]](#footnote-1)**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Fuel Type** | **Units** | **MBtuper Unit** | **CO2elb/MBtu** | **NOxlb/MBtu** | **SO2lb/MBtu** |
| Natural Gas | Therm | 0.1000 | 147.3 | 0.0922 | 0.0006 |
| Fuel Oil #2 | Gallon | 0.1385 | 195.9 | 0.1300 | 0.0015 |
| Liquid Petroleum Gas (LPG) | Gallon | 0.0915 | 177.8 | 0.1421 | 0.0002 |

1. (Informative Note) Developed from ASHRAE Standard 189.1-2020, Addendum m, Appendix J, Table J-6 using combined pre-combustion and combustion values for 100-year GWP time horizon~~the U.S. EPA AP 42, Fifth Edition Compilation of Air Pollutant Emissions Factors, Volume 1, Chapter 1: External Combustion Sources.~~ [~~https://www.epa.gov/air-emissions-factors-and-quantification/ap-42-fifth-edition-volume-i-chapter-1-external-0~~](https://www.epa.gov/air-emissions-factors-and-quantification/ap-42-fifth-edition-volume-i-chapter-1-external-0) [↑](#footnote-ref-1)