**Comment/Explanation\*:***Include your justification for your proposed change to the draft standard below.*
\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

The proposed text edits below reflect a couple of important issues:

* In some cases dimensions are not what is used to determine a quantity. This should be removed.
* 5.6 – the last sentence is limiting. This should not be prohibited.

**Proposed Change to the Draft Standard\***
*Use “strikethrough” and “underline” formatting to indicate all proposed changes. Changes must be shown with “hard-formatting” strikethrough and underline, not “track changes”.*

*Use a color other than red to indicate proposed changes to the draft.*\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

## 5.5 Establishing a Material Inventory

Building *construction documents* shall be used to ~~determine all dimensions required to~~ establish a material inventory for all *Minimum Assessed Products* according to Tables 10.1.1 and 10.1.5.

### For prefabricated components, manufacturer specifications and/or bills of materials are allowed to be used to determine a material inventory according to the requirements of Table 10.1.1.

## *5.6 Existing Home Retrofit* Scenarios

Only newly installed building products shall be included in assessments for retrofit projects. Retained elements shall not contribute to the assessment. *Existing home retrofit* assessments shall use the calculation procedures in this Standard for all *Minimum Assessed Products* included in Table 5.4.1 applied in the retrofit project.

~~Emissions attributed to demolition work and disposal of materials removed from an existing home retrofit assessment shall not be reported.~~