COMMENT 3 (Section 3.2)

Comparable Product Type – Building products that are identical or equivalent to the reference product in terms of composition, functional capabilities, applicable performance attributes, and ability to satisfy applicable code requirements.

REASON:  Performance attributes tend to address intrinsic properties of a material (such as density, compressive strength, etc. etc.) and do not necessarily speak to the functions or multiple functions of a given product that may make it unique or different from others of a similar kind.  For comparability, a comparable product must have comparable functional capabilities, not just comparable performance attributes.  For example, an insulation material will have GWP in functional units (e.g., kgCO2e/RSI-m2), but R-value is not the only function of many insulation materials and it would be inappropriate to consider them as comparable just on the basis of having a common “applicable” performance attribute (R-value).

