COMMENT 7 (only if comments 5 and 6 are both rejected)

Add the following paragraph to Section 10.5 Limitations of This Methodology (Informative):

This standard excludes consideration of directly attributable operational (energy-related) emissions savings of products that have a primary function of energy conservation, like insulation products.  Separate methods to assess the inextricably linked operational emission reductions of such products, like the RESNET 301 standard’s CO2 Index, do not directly attribute any amount of the relative CO2 index value ( or actual operational emissions) to insulation materials nor does it do it in a way that is associated with the full amount of insulation (as counted in this standard for embodied carbon assessment) because the CO2 Index is benchmarked to a 2004 building already having some amount of insulation. Thus, this standard and the CO2 Index, even when used together, do not provide a means to assess the full or total carbon profile of energy conservation products, like insulation.  Therefore, the user must consider the interaction of both embodied carbon emissions and operational (energy-related) emissions by separate means. Such information and guidance may be addressed as additional environmental information in insulation product EPDs.  For additional information, see Product Category Rules (PCR) Guidance for Building-Related Products and Services Part B: Building Envelope Thermal Insulation EPD Requirements, UL 10010-1, Edition 4.0, November 3, 2025).

REASON:  Refer to reason and data provided with Comment #6 (similar rationale).


